Functionality of a program for testing USB - RS232:

1. Choose two COM ports for testing, use 115200 baud rate.
2. Write to TxD1, receive at RxD2, 10 kB packet of random data, compare, and vice versa.
3. Set DTR1, check DCD2, DSR2, and vice versa.
4. Set RTS1, check CTS2, RI2, and vice versa.